**Allied products : Technical data sheet**

**PTW SERIES**

**PTW** **Series** is water base ink for screen printing

**Typical properties**

**Appearance** : Colored viscous paste

**pH** : 8.5

**Scratch hardness** : Good

**Storage stability** : At least 180 days

**Storage** : Should be kept in tightly closed container at

 room temperature, avoid exposure to direct

 sunlight.

**Salient features**

**PTW** **Series** is based on high quality pigment and specialty resins.

**PTW** **Series** has good printing properties when printed full or half tone.

**PTW** **Series** gives good adhesion to the surface.

**PTW** **Series** is free from any additives or fillers.

Greasy / oily surface of the insole should be wiped properly with solvent butyl acetate before applying **PTW** **Series** to get optimum result.

**PTW** **Series** is non hazardous and eco-friendly product.

**Availability**

 **PTW Series** is available in all basic colors.

(without warranty)

For more details please contact:

**Dhupar Chemicals Pvt. Ltd.**

7/82, Tilak Nagar, Kanpur-208002 (India)

Tel: +91-512-2526558,2542795,2557874

E-mail: dhupar@dhuparchemicals.co.in

Web Site: www.dhuparchemicals.co.in Rev. 17/09